|  |  |  |
| --- | --- | --- |
| Command code | Command name | Description |
| 0x01 | READ\_ALL | request for sending all available data |
| 0x03 | ACKNOWLEDGED | positive answer |
| 0x05 | STILL\_AWAKE | check, if workstation is still listening |
| 0x07 | EOF | end of file |
| 0x09 | DATA\_ERR | error in parity bit, or CRC, can be an answer to STILL\_AWAKE or EOT results in all the data transmissions since the last check, being sent again |
| 0x0B | Placeholder for configuration command | placeholder for configuration command |
| 0x0D | Placeholder for configuration command | placeholder for configuration command |
| 0x0F | Placeholder for configuration command | placeholder for configuration command |
| 0x11 | Placeholder for configuration command | placeholder for configuration command |
| 0x13 | Placeholder for configuration command | placeholder for configuration command |
| 0x15 | RESET | used for resetting the MCU |

Overview of all command codes